



	
	
	


Product Guide Specification
Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on MasterFormat 2016 and The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy. 
The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code.  Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” after editing this section. 










Section 28 21 00: Video Surveillance
Section 28 21 11: Analog Cameras

Splicing Controller
 
PART 1 – GENERAL 

1.1 SUMMARY
A. Section Includes
1. Section 28 21 17: Video Surveillance – Surveillance Cameras – Camera Housings
2. Section 28 21 19: Video Surveillance – Surveillance Cameras – Camera Mounts
3. Section 28 27 00: Video Surveillance – Video Surveillance Sensors
B. Related Sections
1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].
2. 
********** Specifier’s note: Include those standards referenced elsewhere in this SECTION.


1.2 REFERENCES
	STANDARD
	NA




1.3 QUALITY ASSURANCE

A. Manufacturer:
1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices.

B. Video Surveillance System:
1. List certifying bodies (CE, FCC, etc.)
2. Provide evidence of compliance upon request.

C. Installer:
1. Minimum of [5] years of experience installing Video Surveillance System.
1.4 DELIVERY, STORAGE AND HANDLING 

A. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels. 

B. Protect store materials from environmental and temperature conditions following manufacturer’s instructions. 

C. Handle and operate products and systems according to manufacturer’s instructions.


1.5 INSTALLATION REQUIREMENTS

A. Operating Temperature And Humidity

B. Power Requirements

1.6 WARRANTY

A. Provide manufacturer’s warranty covering [2] years for replacement and repair of defective equipment. Warranty varies country to country. 


1.7 MAINTENANCE 

A. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.

B. Provide factory direct technical support via phone and e-mail.




PART 2 – PRODUCTS

2.1 MANUFACTURERS

A. Acceptable Manufacturer:
[bookmark: _GoBack]ZHEJIANG DAHUA VISION TECHNOLOGY CO., LTD. 
Address: No.1399, Binxing Road, Binjiang District, Hangzhou, P.R. China
Postcode: 310053
Tel: +86-571-87688888 28933188
Email: dhoverseas@dhvisiontech.com
Website: www.dahuasecurity.com

B. Substitutions:
1. [All proposed substitutions must be approved by the Architect or Engineer professional.]
2. [Proposed substitutions must provide a line-by-line compliance documentation.]

2.2 Splicing Controller | DHI-DSCON2100-0412H
	System
	Main Processor
	High-performance embedded processor

	System
	Operating System
	Embedded Linux

	Function
	Number of Video Output Channels
	12-ch HDMI

	Function
	Interoperability
	ONVIF; Hikvision Private; Dahua Private; GB28181

	Function
	Audio Compression
	PCM; G.711

	Function
	Decoding Capability
	H.264 shares the same decoding with H.265;
Decodes up to 1-ch 32 MP@30 fps, 2-ch 12 MP@30 fps, 4-ch 8 MP@30 fps, 5-ch 6 MP@30 fps, 8-ch 4 MP@30 fps, 16-ch 2 MP@30 fps, and is backward compatible

	Function
	Decoding Pixel
	QCIF; CIF; 2CIF; HD1; D1; 960H; 720p; 1080p; 3 MP; 4 MP; 5 MP; 6 MP; 8 MP; 12 MP; 32 MP

	Function
	Output Resolution
	The default resolution is 1920 × 1080@60 Hz. Supports 1024 × 768@60 Hz, 1280 × 720@60 Hz, 1280 ×1024@60 Hz, 1366 × 768@60 Hz, 1400 × 1050@60 Hz, 1600 ×900@60 Hz, and 1920 × 1080@60 Hz;
It also supports custom resolution output. The width can range from 128 to 3,840, and the height from 128 to 3,840. For custom resolution, it supports up to 3840 × 524@60 Hz or 524 × 3840@60 Hz

	Function
	Video Input
	Supports 2-ch HDMI 2.0, 2-ch HDMI 1.3, and has 3 input modes. It also supports 1-ch 3840 × 2160@60 Hz or 2-ch 3840 × 2160@30 Hz or 4-ch 1920 × 1080@60 Hz. Supports the custom EDID

	Function
	Splicing
	Up to 12 screens can be spliced together

	Function
	Screen Splicing
	Up to 12 screens can be spliced together

	Function
	Window & Roam
	Opens up to 108 windows and supports roaming

	Function
	Scheme Tour
	Supports configuring schemes, tour, scheduled schemes and setting the tour interval

	Function
	Fine Pixel Pitch LED
	The video output resolution can be customized and its fine pixel pitch LEDs can be accessed

	Function
	Background Image Color
	Displays high-definition background images, and supports setting the default background color for the video wall

	Function
	Virtual LED
	Displays customized OSD text, such as the location, font size, and scrolling direction

	Function
	Input Resolution
	The HDMI 2.0 port supports the following resolutions: 3840 × 2160@60 Hz, 3840 × 2160@30 Hz, 2560 × 1440@60 Hz, 1920 × 1080@60 Hz, 1600×900@60 Hz, 1366 × 768@60 Hz, 1024 × 768@60 Hz, and 800 × 600@60 Hz;
The HDMI 2.0 port supports custom resolutions. The width can be 600–4,092, and the height from 400–4,092;
The HDMI 1.3 port supports the following resolutions: 1920 × 1080@60 Hz, 1600 × 900@60 Hz, 1366 × 768@60 Hz, 1024 × 768@60 Hz, and 800 × 600@60 Hz;
The HDMI 1.3 port supports custom resolutions. The width can be 600–2,560, and the height from 400–2,560

	Port
	Video Output
	12-ch HDMI 1.3

	Port
	Audio Output
	1-ch 3.5 mm plug

	Port
	Alarm Input
	1 channel

	Port
	Alarm Output
	1 channel

	Port
	Network Port
	1 × RJ-45 10/100/1,000 Mbps self-adaptive Ethernet port

	Port
	RS-232
	2 × RJ-45 port

	Port
	USB
	3 × USB port

	Port
	RS-485
	1

	General
	Power Supply
	100–240 VAC, 50/60 Hz

	General
	Power Consumption
	≤60 W

	General
	Operating Temperature
	–10 °C to +55 °C (+14 °F to +131 °F)

	General
	Operating Humidity
	10%–95% (RH), non-condensing, 86 kPa–106 kPa

	General
	Product Dimensions
	66 mm × 440 mm × 321 mm (2.60" × 17.32" × 12.64") (H × W × D)

	General
	Packaging Dimensions
	572 mm × 482 mm × 192 mm (22.52" × 18.98" × 7.56") (L × W × H)

	General
	Gross Weight
	7.36 kg (16.23 lb)

	General
	Net Weight
	4.64 kg (10.23 lb)


PART 3 – EXECUTION

3.1 EXAMINATION

A. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
B. Do not begin installation until unacceptable conditions are corrected. 

3.2 PREPARATION

A. Protect devices from damage during construction.

3.3 INSTALLATION

A. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
B. Perform installation with qualified service personnel.
C. Install devices in accordance with the National Electrical Code or applicable local codes.
D. Ensure selected location is secure and offers protection from accidental damage.
E. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference. 

3.4 FIELD QUALITY CONTROL

A. Test snugness of mounting screws of all installed equipment.
B. Test proper operation of all video system devices.
C. Determine and report all problems to the manufacturer’s customer service department.

3.5 ADJUSTING

A. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
B. Make any adjustment of camera settings to comply with specific customer’s need. 

3.6 DEMOSTRATION

A. Demonstrate at final inspection that video management system and devices functions properly.
END OF SECTION
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