



	
	


Product Guide Specification
Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on MasterFormat 2016 and The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy. 
The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code.  Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” after editing this section. 










Section 28 21 00: Video Surveillance
Section 28 21 13: IP Cameras

LCD Digital Signage

PART 1 – GENERAL 

1.1 SUMMARY
A. Section Includes
1. Section 28 21 17: Video Surveillance – Surveillance Cameras – Camera Housings
2. Section 28 21 19: Video Surveillance – Surveillance Cameras – Camera Mounts
3. Section 28 27 00: Video Surveillance – Video Surveillance Sensors
B. Related Sections
1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].
2. 
********** Specifier’s note: Include those standards referenced elsewhere in this SECTION. 

1.2 REFERENCES
	STANDARD
	CE EMC, CE LVD, CE ERP, RED



1.3 SYSTEM DESCRIPTION

A. Section Includes
1. Video Surveillance – Surveillance Cameras –LCD Digital Signage
1.4 SUBMITTALS

A. 	Product Data: 
1. Manufacturer’s data, user and installation manuals for all equipment and software programs including computer equipment and other equipment required for complete video management system. 
B. Dimensional Drawings; include
1. Overall device dimensions. 
2. Dimensions specific for installation. 
C. Closeout Submittals
1. User manual.
2. Parts list.
3. Maintenance requirements.

1.5 QUALITY ASSURANCE

A. Manufacturer: 
1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices. 
B. Video Surveillance System: 
1. List certifying bodies (UL, etc.) 
2. Provide evidence of compliance upon request. 
C. Installer: 
1. Minimum of [5] years of experience installing Video Surveillance System. 

1.6 DELIVERY, STORAGE AND HANDLING 

A. Comply with requirements of Section 01 60 00. 
B. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels. 
C. Protect store materials from environmental and temperature conditions following manufacturer’s instructions. 
D. Handle and operate products and systems according to manufacturer’s instructions. 

1.7 WARRANTY

A. Provide manufacturer’s warranty covering [3] years for replacement and repair of defective equipment. Warranty varies country to country.


1.8 MAINTENANCE 

A. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users. 
B. Provide factory direct technical support via phone and e-mail. 

PART 2 – PRODUCTS

2.1 MANUFACTURERS

A. Acceptable Manufacturer: 
[bookmark: _GoBack]ZHEJIANG DAHUA VISION TECHNOLOGY CO., LTD. 
Address: No.1399, Binxing Road, Binjiang District, Hangzhou, P.R. China
Postcode: 310053
Tel: +86-571-87688888 28933188
Email: dhoverseas@dhvisiontech.com
Website: www.dahuasecurity.com

B. Substitutions: 
1. [All proposed substitutions must be approved by the Architect or Engineer professional.] 
2. [Proposed substitutions must provide a line-by-line compliance documentation.] 

2.2 LCD Digital Signage | DHI-LDH43-HAI400L-V2
	LCD Panel
	Screen Size
	43 inch

	LCD Panel
	Backlight
	ELED

	LCD Panel
	LCD Technology
	IPS/VA

	LCD Panel
	Aspect Ratio
	16:9

	LCD Panel
	Brightness
	700 cd/m² (typ.)

	LCD Panel
	Contrast Ratio
	IPS 1200:1 (typ.) / VA 4000:1 (typ.)

	LCD Panel
	Display Colors
	10 bit (8 bit + FRC), 1.07B colors

	LCD Panel
	Resolution
	3840 (H) × 2160 (V)

	LCD Panel
	Viewing Angle
	178° (H)/178° (V)

	LCD Panel
	Response Time
	8 ms

	LCD Panel
	Surface Treatment
	Haze 25%

	Built-in System
	Operating System
	Android 11.0

	Built-in System
	CPU
	4 cores A55, 1.92 GHz

	Built-in System
	RAM
	4 GB

	Built-in System
	ROM
	32 GB

	Built-in System
	Video Decoding
	H.265 HEVC MP-10@L5.1 up to 2160p@60 fps;
H.264 AVC HP@L5.1 up to 2160p@30 fps;
VP9 Profile 2 up to 2160p@60 fps; 
H.264 MVC up to 1080p@30 fps; 
MPEG-4 ASP@L5 up to 1080p@30 fps;
WMV/VC-1 SP/MP/AP up to 1080p@30 fps;

	Function
	Audio Compression
	MPEG-3, WMA, WAV

	Function
	Video Compression
	MPEG-4, H.264 AVC/MVC, H.265 HEVC

	Function
	Video Format
	mp4, avi, mov, mkv, wmv

	Device Ports
	Network Port
	1 × RJ–45 10/100/1,000 Mbps self-adaptive Ethernet port

	Device Ports
	Wi-Fi Standard
	802.11 b/g/n/a/ac/ax

	Device Ports
	Wi-Fi Frequency Range
	2400-2483.5 MHz, 5150-5350 MHz, 5470-5725 MHz, 5725-5850 MHz

	Device Ports
	MAX Power Transmission (Wi-Fi)
	≤20 dBm@2400-2483.5 MHz;
≤23 dBm@5150-5250 MHz;
≤20 dBm@5250-5350 MHz;
≤27 dBm@5470-5725 MHz;
≤14 dBm@5725-5850 MHz

	Device Ports
	Data Transmission Ports
	1 × USB 2.0 (type A); 1 × USB 3.0 (type A)
1 × TF card slot, up to 128 GB

	Device Ports
	Video Input
	1 × HDMI 2.1 (4K@60 Hz)

	Device Ports
	Audio Port
	1 × 3.5 mm jack output

	Speaker
	Built-in Speaker
	2 × 5 W

	General
	Power Supply
	100–240 VAC, 50/60 Hz

	General
	Power Consumption
	100 W (typ.), 125 W (max)

	General
	Standby Power Consumption
	≤0.5 W

	General
	Operating Temperature
	0 °C to +40 °C (+32 °F to +104 °F) (avoid direct sunlight)

	General
	Storage Temperature
	–20 °C to +60 °C (–4 °F to +140 °F)

	General
	Operating Humidity
	10%–85% (RH), non-condensing

	General
	Storage Humidity
	10%–90% (RH), non-condensing

	General
	Product Material
	Metal casing

	General
	Casing Color (Frame/Rear)
	Black

	General
	Product Dimensions
	964.6 mm × 552.9 mm × 25.0 mm (37.98" × 21.77" × 0.98") (L × H × W) (without bracket)
964.6 mm × 552.9 mm × 27.5 mm (37.98" × 21.77" × 1.08") (L × H × W) (with bracket)

	General
	Frame Size
	10.3 mm (0.41") (T/L/R/B)

	General
	Packaging Dimensions
	1,056 mm × 130 mm × 652 mm (41.57" × 5.12" × 25.67") (L × W × H)

	General
	Net Weight
	13.0 kg (28.66 lb)

	General
	Gross Weight
	16.5 kg (36.38 lb)

	General
	Wall Mount VESA
	400 mm × 400 mm (15.75" × 15.75")

	General
	Installation
	Wall mount

	General
	Display Mode
	Landscape/Portrait

	General
	Accessory
	Wall-mount bracket, user manual, legal and regulatory information, energy label, remote control


PART 3 – EXECUTION

3.1 EXAMINATION

A. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation. 
B. Do not begin installation until unacceptable conditions are corrected. 

3.2 PREPARATION

A. Protect devices from damage during construction.

3.3 INSTALLATION

A. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
B. Perform installation with qualified service personnel. 
C. Install devices in accordance with the National Electrical Code or applicable local codes.
D. Ensure selected location is secure and offers protection from accidental damage.
E. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference. 

3.4 FIELD QUALITY CONTROL

A. Test snugness of mounting screws of all installed equipment. 
B. Test proper operation of all video system devices. 
C. Determine and report all problems to the manufacturer’s customer service department. 

3.5 ADJUSTING

A. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions. 
B. Make any adjustment of camera settings to comply with specific customer’s need. 

3.6 DEMOSTRATION

A. Demonstrate at final inspection that video management system and devices functions properly. 
END OF SECTION
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