



	
	
	


Product Guide Specification
Specifier Notes:  This product guide specification is written according to the Construction Specifications Institute (CSI) 3-Part Format, based on MasterFormat 2016 and The Project Resource Manual—CSI Manual of Practice. The Manufacturer is responsible for technical accuracy. 
The section must be carefully reviewed and edited by the Architect or Engineer to meet the requirements of the project and local building code.  Words and sentences within brackets [ ] are choices to include or exclude a particular item or statement.  Coordinate this section with other specification sections and the Drawings.  Delete all “Specifier Notes” after editing this section. 










Section 28 21 00: Video Surveillance
Section 28 21 11: Analog Cameras

NETWORK VIDEO DECODER
 
PART 1 – GENERAL 

1.1 SUMMARY
A. Section Includes
1. Section 28 21 17: Video Surveillance – Surveillance Cameras – Camera Housings
2. Section 28 21 19: Video Surveillance – Surveillance Cameras – Camera Mounts
3. Section 28 27 00: Video Surveillance – Video Surveillance Sensors
B. Related Sections
1. [Section 28 33 15: Security Detection, Alarm and Monitoring – Security Monitoring and Control – Security Monitoring and Control Software].
2. 
********** Specifier’s note: Include those standards referenced elsewhere in this SECTION.


1.2 REFERENCES
	STANDARD
	CE LVD: SHES2211021486AT;
CE EMC: KSEM2211002215Ver;
FCC: 4789974549-2




1.3 QUALITY ASSURANCE

A. Manufacturer:
1. Minimum of [10] years of experience in manufacture and design Video Surveillance Devices.

B. Video Surveillance System:
1. List certifying bodies (CE, FCC, etc.)
2. Provide evidence of compliance upon request.

C. Installer:
1. Minimum of [5] years of experience installing Video Surveillance System.
1.4 DELIVERY, STORAGE AND HANDLING 

A. Deliver materials in manufacture’s original, unopened, undamaged containers; and unharmed original identification labels. 

B. Protect store materials from environmental and temperature conditions following manufacturer’s instructions. 

C. Handle and operate products and systems according to manufacturer’s instructions.


1.5 INSTALLATION REQUIREMENTS

A. Operating Temperature And Humidity

B. Power Requirements

1.6 WARRANTY

A. Provide manufacturer’s warranty covering [2] years for replacement and repair of defective equipment. Warranty varies country to country. 


1.7 MAINTENANCE 

A. Make ordering of new equipment for expansions, replacements, and spare parts available to dealers and end users.

B. Provide factory direct technical support via phone and e-mail.




PART 2 – PRODUCTS

2.1 MANUFACTURERS

A. Acceptable Manufacturer:
[bookmark: _GoBack]ZHEJIANG DAHUA VISION TECHNOLOGY CO., LTD. 
Address: No.1399, Binxing Road, Binjiang District, Hangzhou, P.R. China
Postcode: 310053
Tel: +86-571-87688888 28933188
Email: dhoverseas@dhvisiontech.com
Website: www.dahuasecurity.com

B. Substitutions:
1. [All proposed substitutions must be approved by the Architect or Engineer professional.]
2. [Proposed substitutions must provide a line-by-line compliance documentation.]

2.2 NETWORK VIDEO DECODER | DHI-NVD0405DU-2I-8K
	System
	Main Processor
	High-performance embedded processor

	System
	Operating System
	Embedded Linux

	Function
	Number of Video Output Channels
	4 × HDMI

	Function
	Video Compression
	H.265; H.264; MJPEG; MPEG4; SVAC; MPEG2

	Function
	Decoding Capability
	Supports maximum 2-ch 32MP@25 fps videos, 7-ch 12MP@25 fps, 10-ch 8MP@25 fps videos, 14-ch 6MP@25 fps videos, 18-ch 5MP@25 fps videos, 28-ch 3MP@25 fps videos, 36-ch 1080p@30 fps videos and 144-ch D1@30 fps decoded at the same time

	Function
	Output Resolution
	1024 × 768, 1280 × 720, 1280 × 1024, 1920 × 1080, 1920 × 1200, 2048 × 1152, 3840 × 2160 @30Hz, 3840 × 2160@60 Hz, 4096 × 2160@24 Hz. It is 1920 × 1080 by default

	Function
	Video Input
	2 × HDMI

	Function
	Screen Splicing
	Up to 4 windows can be spliced together

	Function
	Window & Roam
	Supports customized windowing and roaming. Up to 36 channels with windowing

	Function
	Scheme Tour
	Supports saving scheme, scheme tour, scheduled scheme, and customizing tour interval

	Function
	Fine Pixel Pitch LED
	Supports customized resolution output and connecting to small-pitch LEDs

	Function
	Background Image Color
	Supports configuring the background image color of the video wall and displaying HD images

	Function
	Enable AI Function
	Displays intelligent streams on the video wall, such as face, human, motor vehicle, non-motor vehicle, crowd density and intelligent rules

	Function
	Virtual LED
	Displays customized OSD text, such as location and font size

	Function
	Input Resolution
	800 × 600, 1024 × 768, 1280 × 720, 1280 × 800, 1280 × 960, 1280 × 1024, 1440 × 900, 1680 × 1050, 1920 × 1080, 3840 × 2160@30 Hz and 3840 × 2160@60 Hz

	Port
	Video Output
	4 × HDMI

	Port
	Audio Output
	1 × 3.5 mm

	Port
	Alarm Input
	8

	Port
	Alarm Output
	8

	Port
	Network Port
	1 × RJ–45 10 M/100 M/1000 M self-adaptive Ethernet port

	Port
	RS-232
	2 (1 × DB9, 1 × RJ-45)

	Port
	USB
	3 × USB (1 for the front panel, 2 for the back panel)

	Port
	RS-485
	1

	General
	Power Supply
	12 VDC

	General
	Power Consumption
	≤60 W

	General
	Operating Temperature
	–10 °C to +55 °C (+14 °F to +131 °F)

	General
	Operating Humidity
	10%–95% (RH), non-condensing (86 kPa–106 kPa)

	General
	Product Dimensions
	440 mm × 322 mm × 44 mm (17.32" × 12.68" × 1.73") (L × W × H) (1U height)

	General
	Packaging Dimensions
	140 mm × 402 mm × 536 mm (5.51" × 15.83" × 21.10") (H × W × D)

	General
	Gross Weight
	4.9 kg–5.2 kg (10.80 lb–11.46 lb)

	General
	Net Weight
	3.2 kg–3.5 kg (7.05 lb–7.72 lb)


PART 3 – EXECUTION

3.1 EXAMINATION

A. Examine areas to receive devices and notify adverse conditions affecting installation or subsequent operation.
B. Do not begin installation until unacceptable conditions are corrected. 

3.2 PREPARATION

A. Protect devices from damage during construction.

3.3 INSTALLATION

A. Install devices in accordance with manufacturer’s instruction at locations indicated on the floor drawings plans.
B. Perform installation with qualified service personnel.
C. Install devices in accordance with the National Electrical Code or applicable local codes.
D. Ensure selected location is secure and offers protection from accidental damage.
E. Location must provide reasonable temperature and humidity conditions, free from sources of electrical and electromagnetic interference. 

3.4 FIELD QUALITY CONTROL

A. Test snugness of mounting screws of all installed equipment.
B. Test proper operation of all video system devices.
C. Determine and report all problems to the manufacturer’s customer service department.

3.5 ADJUSTING

A. Make proper adjustment to video system devices for correct operation in accordance with manufacturer’s instructions.
B. Make any adjustment of camera settings to comply with specific customer’s need. 

3.6 DEMOSTRATION

A. Demonstrate at final inspection that video management system and devices functions properly.
END OF SECTION
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